**SBC65 V0 EEPROM Configuration**

**Format**

|  |  |  |
| --- | --- | --- |
| ID | word | identifier |
| length | word | Length of entry in bytes |
| DATA | N bytes | Data entry |

**Identifier**

|  |  |
| --- | --- |
| User Data | $0000 .. $3FFF |
| User Code | $4000 .. $7FFF |
| System Data | $8000 .. $BFFF |
| System Code | $C000 .. $FFFE |
| Last entry | $FFFF |

Identifier Table

|  |  |
| --- | --- |
|  |  |
|  |  |
| $4000 | Erase 24C32, start adr $130, length $7A |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |